External Forward Caller-ID

If the carrier fails the external forward because of the order in which caller id is presented the code ;3E

Will flip the entry presentation.

Reference names, Maxreal and Marty Lee Soraa, Comcast trunks